
Application of EC-8

## Step1: Seismic Zone – Based on hazard mapA map of france with different colored areas Description automatically generated

## Step 2: Reference peak ground acceleration on type A ground, agR



## Step 3: Soil Class

A white sheet with black text

Description automatically generated

## Step 4: Category of importance

**Arrêté 22/10/2010 mod. 18/07/2011 - Article 2 : Catégories d'importance des bâtiments**

A close-up of a document

Description automatically generated

## Step 5: Criteria for structural regularity

…